The MC68HC912D60A microcontroller unit (MCU) is a 16-bit device
available in two package options, 80-pin QFP and 112-pin TQFP. Onchip
peripherals include a 16-bit central processing unit (CPU12), 60K
bytes of flash EEPROM, 2K bytes of RAM, 1K bytes of EEPROM, two
asynchronous serial communication interfaces (SCI), a serial peripheral
interface (SPI), an enhanced capture timer (ECT), two (one on 80QFP)
8-channel,10-bit analog-to-digital converters (ATD), a four-channel
pulse-width modulator (PWM), and a CAN 2.0 A, B software compatible
module (MSCAN12).