The MC68HC908GZ60, MC68HC908GZ48, and MC68HC908GZ32 are members 
high-performance M68HC08 Family of 8-bit microcontroller units (MCUs). 
All MCUs in the family use the enhanced M68HC08 central processor unit (CPU08) 
and are available with a variety of modules, memory sizes and types, and package types.



Features of the MC68HC908GZ60 include:
- High-performance M68HC08 architecture optimized for C-compilers
- Fully upward-compatible object code with M6805, M146805, and M68HC05 Families
- 8-MHz internal bus frequency
- Clock generation module supporting 1-MHz to 8-MHz crystals
- MSCAN08 (scalable controller area network) controller (implementing 2.0b protocol as defined in BOSCH specification dated September 1991)
- FLASH program memory security(1)
- On-chip programming firmware for use with host personal computer which does not require high voltage for entry
- In-system programming (ISP)
- System protection features:
- Optional computer operating properly (COP) reset
- Low-voltage detection with optional reset and selectable trip points for 3.3-V and 5.0-V operation
- Illegal opcode detection with reset
- Illegal address detection with reset
- Low-power design; fully static with stop and wait modes

On-chip FLASH memory:
- MC68HC908GZ60 - 60 Kbytes
- MC68HC908GZ48 - 48 Kbytes
- MC68HC908GZ32 - 32 Kbytes
Random-access memory (RAM):
- MC68HC908GZ60 - 2048 bytes
- MC68HC908GZ48 - 1536 bytes
- MC68HC908GZ32 - 1536 bytes
