The 68HC(9)12D60 microcontroller unit (MCU) is a 16-bit device
available in two package options, 80-pin QFP and 112-pin TQFP. Onchip
peripherals include a 16-bit central processing unit (CPU12), 60K
bytes of flash EEPROM (68HC912D60) or ROM (68HC12D60), 2K
bytes of RAM, 1K bytes of EEPROM, two asynchronous serial
communication interfaces (SCI), a serial peripheral interface (SPI), an
enhanced capture timer (ECT), two (one on 80QFP) 8-channel,10-bit
analog-to-digital converters (ATD), a four-channel pulse-width
modulator (PWM), and a CAN 2.0 A, B software compatible module
(MSCAN12).


The Flash EEPROM module requires an external program/erase voltage
(VFP) to program or erase the Flash EEPROM array.