24C08 - I2C (2-Wire) Serial EEPROM

Features
* Low Voltage and Standard Voltage Operation
* Internally Organized 1024 x 8
* 2-Wire Serial Interface
* Bidirectional Data Transfer Protocol
* 100 kHz (1.8V - 2.7V) and 400 kHz (5V) Compatibility
* 4-Byte Page Write Mode
* Self-Timed Write Cycle (10 ms max)
* High Reliability
* Endurance: 1 Million Write Cycles
* 8-Pin PDIP, 8-Pin MSOP, 8-Pin TSSOP and 8-Pin JEDEC SOIC Packages

Pin Description
SERIAL CLOCK (SCL): The SCL input is used to positive
edge clock data into each EEPROM device and negative
edge clock data out of each device.
SERIAL DATA (SDA): The SDA pin is bidirectional for
serial data transfer. This pin is open-drain driven and may
be wire-ORed with any number of other open-drain or open
collector devices.
