24C16 - I2C (2-Wire) Serial EEPROM

Features
* Low-Voltage and Standard-Voltage Operation
* Internally Organized 1024 x 8 
* 2-Wire Serial Interface
* Schmitt Trigger, Filtered Inputs for Noise Suppression
* Bidirectional Data Transfer Protocol
* 100 kHz (1.8V - 2.7V) and 400 kHz (5V) Compatibility
* Write Protect Pin for Hardware Data Protection
* 16-Byte Page Write Modes
* Partial Page Writes Are Allowed
* Self-Timed Write Cycle (10 ms max)
* High Reliability
* Endurance: 1 Million Write Cycles
* Data Retention: 100 Years
* 8-Pin and 14-Pin JEDEC SOIC, 8-Pin PDIP, 8-Pin MSOP, and 8-Pin TSSOP Packages

Pin Description
SERIAL CLOCK (SCL): The SCL input is used to positive
edge clock data into each EEPROM device and negative
edge clock data out of each device.
SERIAL DATA (SDA): The SDA pin is bidirectional for
serial data transfer. This pin is open-drain driven and may
be wire-ORed with any number of other open-drain or open
collector devices.
