PIC18F2XJXX/4XJXX FAMILY

12V to MCLR not reqired.

The last eight bytes of the code space
(also called the Flash Configuration Words) 
should be written with configuration data and not executable code.