ST M35080
8 Kbit Serial SPI Bus EEPROM With Incremental Registers

- Compatible with SPI Bus Serial Interface (Positive Clock SPI Modes)
- Single Supply Voltage: 4.5 V to 5.5 V
- 5 MHz Clock Rate (maximum)
- Sixteen 16-bit Incremental Registers
- Hardware Protection of the Status Register
- Resizeable Read-Only EEPROM Area