The 08AS60/AZ60 is a member of the low-cost, high-performance
M68HC08 Family of 8-bit microcontroller units (MCU). The M68HC08
Family is based on the customer-specified integrated circuit (CSIC)
design strategy. All MCUs in the family use the enhanced M68HC08
central processor unit (CPU08) and are available with a variety of
modules, memory sizes and types, and package types.
This part is designed to emulate the M68HC08ASxx automotive family.

Default FLASH state - 00

For activate security set 0D3H to EEPROM address 0200H.

For read FLASH skip and deactivate security,
select 908AZ60 and serach SS.